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	Unité magnétique - 3xN52-Ø52,4 mm - SECA3030

Nº d'article: E0103537



Caractéristiques techniques
	La description
	Unité magnétique - 3xN52-Ø52,4 mm - SECA3030

	Nº d'article
	E0103537

	Clé de produit
	SECA-S-3030-03V-ES MAGNET INSE

	Product name
	Cleanflow - automatic discontinuouosly cleaning insert                

	Suitable for food production
	For non-perishable foods only                

	Max. particle size
	10 mm                

	Min. Fe-particle size that can be caught
	0,03 mm                

	Production stop required during ferrous particles disposal
	Yes                

	Cleaning (ferrous particles disposal) method
	Automatic                

	Pneumatic connection
	For 6 mm hose                

	Materials in contact with product
	AISI304 (SS 1.4301) / AISI316L (SS 1.4404)                

	Material seal rings between housing and magnetic bars
	Silicone 714177 coated, 70° Shore, EC1935/FDA, red                

	Surface finishing (interior/exterior)
	S5: Polished, Ra 0.4 Âµm, excl. welds & end faces                

	Max. operating temperature
	80 °C                

	Min./max. ambient temperature
	-10 to 60 °C                

	Magnetic system
	Magnetic bar in tube                

	Magnet quality
	Neodymium N-52                

	Magnetic bar size
	Ø52,4 mm (wall thickness 1,2 mm)                

	Number of magnetic bars
	3                

	Flux density on magnet tube in contact with product (±10%)
	12000 gauss                

	Control
	Pneumatic                

	Length
	781 mm                

	Width
	470 mm                

	Height
	111 mm                

	Weight
	38 kg                
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