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	Elektromagnetyczny separator podwieszany - 700 mm

Numer artykułu: SEBM020001



Właściwości
	Opis
	Elektromagnetyczny separator podwieszany - 700 mm

	Numer artykułu
	SEBM020001

	Klucz produktu
	RBE-EP5-062x070-070-A-NA

	Min. Fe-particle size that can be caught
	3 mm                

	Advised max. installation height
	170-240 mm                

	Production stop required during ferrous particles disposal
	Yes                

	Cleaning (ferrous particles disposal) method
	Automatic                

	Ferrous particles disposal via
	By switching off electromagnet                

	Suitable for belt width
	700 mm                

	Installation/transport interface
	Lifting eye Ø40 mm (4x)                

	Material housing
	Steel                

	Surface treatment/finishing
	Painted                

	Colour housing
	Blue (Ultramarine blue): RAL 5002                

	Max. operating temperature
	80 °C                

	Min./max. ambient temperature
	-10 to 40 °C                

	Dust/water protection class
	IP54                

	Magnetic system
	Electromagnet with air cooling                

	Magnet power
	2000 W                

	Magnet current
	25 A                

	Magnet voltage
	80 V DC                

	Duty cycle
	100%, 24 hours/day                

	Associated control unit (not included)
	ESBB902001                

	Length
	798 mm                

	Width
	630 mm                

	Height
	413 mm                

	Weight
	750 kg                
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