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	Control box - 400 V AC + N + PE; 50/60 Hz

Article number: E0122431



Attributes
	Description
	Control box - 400 V AC + N + PE; 50/60 Hz

	Article number
	E0122431

	Product key
	RHPS-E-CB-NA-LC-HW-FD1

	Control box type
	Wall mounted                

	Suitable for
	High-gradient magnetic head pulley system / Overband magnet                

	Surface treatment/finishing
	Powder-coated, textured paint (exterior)                

	Colour
	Grey (Light grey): RAL7035                

	Min./max. ambient temperature
	-10 to 30 °C                

	Dust/water protection class
	IP54                

	EMC directive 2014/30/EU compliant
	EMC_2014-30EU                

	EN 60204-1 compliant
	Yes                

	EN ISO 13849-1 compliant
	Yes                

	EN ISO 13850 compliant
	Yes                

	IEC 61439-1 compliant
	Yes                

	IEC 61439-2 compliant
	Yes                

	Supply voltage
	3x400 V AC + N + PE; 50 Hz                

	Supply current
	16 A                

	Maximum fuse
	16 A                

	Output power
	4,7 kW                

	Output power to belt drive
	0,37 kW                

	Output voltage to belt drive
	400 V AC                

	Output current to belt drive
	1,1 A                

	Output power to vibr. feeder
	2 x 0,2 kW                

	Output power to overband magnet
	1,5 kW                

	Output voltage to overband magnet
	400 V AC                

	Output current to overband magnet
	Max. 4,7 A                

	Incl. pot. free contacts for PLC
	Yes                

	Including plug connection between control box and cable set
	Yes                

	Main switch
	Black/grey                

	Indicator light 'Running' (green)
	Yes                

	Emergency stop
	Yes                

	Push button 'Reset emergency stop'
	Yes                

	Push button ON
	Yes                

	Push button OFF
	Yes                

	Switch for local/remote control
	Yes                

	Potentiometer belt speed
	Yes                

	Potentiometer feeder speed
	Yes                

	Depth
	210 mm                

	Width
	500 mm                

	Height
	500 mm                

	Weight
	25 kg                


www.goudsmitmagnetics.com	Pagina 1 van 2
www.goudsmitmagnetics.com			Page 1 of 2

image1.png
GOWVDSEV

ETICS

AGIN




